{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["表-08_分部分项工程和单价措施项目清单与计价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"表-08_分部分项工程和单价措施项目清单与计价表","index":0,"n_rows":96,"n_cols":5,"rows_kept":96,"merged":[[0,0,0,4],[1,0,1,4],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[3,4,4,4],[36,0,36,4],[37,0,37,4],[38,0,40,0],[38,1,40,1],[38,2,40,2],[38,3,40,3],[39,4,40,4],[73,0,73,4],[74,0,74,4],[75,0,77,0],[75,1,77,1],[75,2,77,2],[75,3,77,3],[76,4,77,4],[94,0,94,4],[95,0,95,4]],"flags":["formulas_cached_only"]}
["部分项目单价最高限价"]
["工程名称:南宁经济技术开发区铁山港西路（铁山港一支路—铁山港三支路）工程                  第1页 共3页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","金额(元)"]
[{"$nulls":4},"综合单价"]
[]
[null,null,"南宁经济技术开发区铁山港西路（铁山港一支路—铁山港三支路）工程-道路工程"]
[null,null,"分部分项工程"]
[null,"0401","土石方工程"]
["2","★040102001001","路基挖石方(含装车)","",20.73]
[null,null,"含：各类石方开挖及爆破，石方类别综合考虑"]
["4","★040103001002","路基借土方回填压实","",16.83]
[null,null,"含：1、回填、压实等，压实度按施工图设计要求"]
[null,null,"    2、借土取土及装运"]
[null,null,"    3、取土运距及购土费：投标人自行考虑"]
[null,null,"    4、土质包括三合土、天然砂砾土、普通土等"]
["5","★040103002001","余土方弃置(含运弃)","",11.44]
[null,null,"含：1、各类土方(包括淤泥、流沙等)，土方类别综合考虑"]
[null,null,"    2、表土、树、竹，树根及竹兜"]
[null,null,"    3、杂草、水葫芦、漂浮物"]
[null,null,"    4、挖深层搅拌桩桩头等"]
[null,null,"    5、运距及弃土场费：投标人自行考虑"]
["6","★040103002002","余石方弃置(含运弃)","",16.99]
[null,null,"含：1、各类石方，石方类别综合考虑"]
[null,null,"    2、砼及钢筋砼结构物、水泥混凝土路面"]
[null,null,"    3、运距及弃土场费：投标人自行考虑"]
[null,"0402","道路工程"]
["14","◆★040201013001","50cm深层搅拌桩","m",34.41]
[null,null,"含：1、水泥掺入量为加固干土重15%，水灰比0.5，水泥土强度大于等于1700kpa"]
[null,null,"    2、桩间距110cm,正三角形布置"]
[null,null,"    3、深层搅拌桩施工工艺：二喷四搅"]
[null,null,"    4、桩身强度及桩距按设计要求"]
[null,null,"    5、具体做法详施工图设计"]
["22","◆★040203006001","7cm厚AC-25C型粗粒式沥青砼底面层","㎡",44.08]
["25","◆★040203006002","5cm厚AC-20C型中粒式沥青砼中面层","㎡",32.65]
["26","◆★040203006003","4cm厚AC-13C型细粒式改性沥青砼上面层","㎡",35.52]
["27","◆★040203006004","4cm厚ARAC-13C型细粒式橡胶改性沥青砼上面层（骨料采用辉绿岩）","㎡",59.56]
["部分项目单价最高限价"]
["工程名称:南宁经济技术开发区铁山港西路（铁山港一支路—铁山港三支路）工程                  第2页 共3页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","金额(元)"]
[{"$nulls":4},"综合单价"]
[]
[null,"0410","拆除工程"]
["41","★041001001001","拆除水泥砼路面（含装车）","",{"v":87,"d":"87.00"}]
["42","★041001008001","拆除建筑物素砼基础(含装车)","",159.07]
[null,null,"南宁经济技术开发区铁山港西路（铁山港一支路—铁山港三支路）工程-排水工程"]
[null,null,"分部分项工程"]
[null,"0401","土石方工程"]
["50","★040102002001","沟槽、基坑挖石方(含装车)","",42.61]
[null,null,"含：各类石方开挖及爆破，石方类别综合考虑"]
["52","★040103001006","沟槽、基坑借土方回填压实","",27.07]
[null,null,"含：1、回填、压实等，压实度和土质按施工图设计要求"]
[null,null,"    2、借土、取土及装运"]
[null,null,"    3、取土运距及购土费：投标人自行考虑"]
["53","★040103002003","余土方弃置(含运弃)","",11.44]
[null,null,"含：1、各类土方(包括淤泥、流沙等)，土方类别综合考虑"]
[null,null,"    2、表土、砍树、竹，挖树根及竹兜"]
[null,null,"    3、杂草、水葫芦、捞漂浮物"]
[null,null,"    4、挖深层搅拌桩桩头等"]
[null,null,"    5、运距及弃土场费：投标人自行考虑"]
["54","★040103002004","余石方弃置(含运弃)","",16.99]
[null,null,"含：1、各类石方，石方类别综合考虑"]
[null,null,"    2、运距及弃土场费：投标人自行考虑"]
[null,null,"南宁经济技术开发区铁山港西路（铁山港一支路—铁山港三支路）工程-照明工程"]
[null,null,"分部分项工程"]
[null,"0408","路灯工程"]
["185","★030412007001","LED单臂灯 1*150W H=11m 臂长2.5m","套",2850.34]
[null,null,"含：1、灯杆采用热镀锌Q235钢板，外表面喷白色塑层，灯杆底板采用25mm厚钢板"]
[null,null,"    2、灯杆配电门采用不可拆卸合页开门方式，并加装防护链，以及采用8内沉头三角螺栓上锁，配路灯开关盒及接地端子"]
[null,null,"    3、灯具为高压铸铝一次成型结构，具有良好的防水性能，防护等级要求≥IP65"]
[null,null,"    4、相适应的电流驱动器、散热模组、灯罩等，电源驱动器要求采用节能型电流驱动器"]
[null,null,"    5、灯具内需密封的部位，必须使用耐高温防老化的硅胶防护圈，不允许使用玻璃棉、海棉泡沫防护胶"]
[null,null,"    6、灯具反光板采用高纯度阳极氧化铝板"]
[null,null,"    7、单臂灯采用一根3*2.5mm铜芯线"]
["部分项目单价最高限价"]
["工程名称:南宁经济技术开发区铁山港西路（铁山港一支路—铁山港三支路）工程                  第3页 共3页"]
["序\r\n\r\n号","项目编码","项目名称及\r\n项目特征描述","计量单位","金额(元)"]
[{"$nulls":4},"综合单价"]
[]
["186","★030412007002","LED二火泛光灯 2*150W H=14m","套",4614.71]
[null,null,"含：1、灯杆采用热镀锌Q235钢板，外表面喷白色塑层，灯杆底板采用25mm厚钢板"]
[null,null,"    2、灯杆配电门采用不可拆卸合页开门方式，并加装防护链，以及采用8内沉头三角螺栓上锁，配路灯开关盒及接地端子"]
[null,null,"    3、灯具为高压铸铝一次成型结构，具有良好的防水性能，防护等级要求≥IP65"]
[null,null,"    4、相适应的电流驱动器、散热模组、灯罩等，电源驱动器要求采用节能型电流驱动器"]
[null,null,"    5、灯具内需密封的部位，必须使用耐高温防老化的硅胶防护圈，不允许使用玻璃棉、海棉泡沫防护胶"]
[null,null,"    6、灯具反光板采用高纯度阳极氧化铝板"]
[null,null,"    7、灯具内配线采用BVVB-0.45/0.75KV双护套铜芯线"]
["187","★030412007003","LED三火泛光灯 3*240W H=14m","套",5358.61]
[null,null,"含：1、灯杆采用热镀锌Q235钢板，外表面喷白色塑层，灯杆底板采用25mm厚钢板"]
[null,null,"    2、灯杆配电门采用不可拆卸合页开门方式，并加装防护链，以及采用8内沉头三角螺栓上锁，配路灯开关盒及接地端子"]
[null,null,"    3、灯具为高压铸铝一次成型结构，具有良好的防水性能，防护等级要求≥IP65"]
[null,null,"    4、相适应的电流驱动器、散热模组、灯罩等，电源驱动器要求采用节能型电流驱动器"]
[null,null,"    5、灯具内需密封的部位，必须使用耐高温防老化的硅胶防护圈，不允许使用玻璃棉、海棉泡沫防护胶"]
[null,null,"    6、灯具反光板采用高纯度阳极氧化铝板"]
[null,null,"    7、灯具内配线采用BVVB-0.45/0.75KV双护套铜芯线"]
["编制单位：广西中信恒泰工程顾问有限公司                                       审核单位：南宁经济技术开发区财政局"]
["日期：二0一六年六月十七日"]